

Wheat and corn arrive through two pipes. The raw material comes from the mixer storage hopper. The system for moving the seeds is carried out by pneumatic energy.

The separating unit of the DMS line. This part is composed of a hopper and a storage unit for wheat and corn.

When wheat and corn arrive in the tray where the hopper is located, a motor makes the sieve vibrate. It then separates the wheat from the corn.



When sorting, the connecting sleeve for wheat and corn opens

The wheat drops on the left part and the corn on the right part, each in a different hopper, before being conveyed to the mixer.

A pipe runs from each compartment to supply the wheat and corn mixer.